**AUDIO SERVER 1 COMPUTER**

OPEN **DANTE VIRTUAL SOUNDCARD**

* Make sure Network Interface is set to Dante (en6)

OPEN Show File: “BW\_Audio Control Patch”

OPEN Master Audio Levels Control: “Bluey Control\_Master\_2”

(for adjusting overall volume of show)

* This is only on Audio Server 1 PC
* Use this to adjust audio levels if someone asks for louder/quieter audio
* Set to 0 for weekends/busy days and -3 for weekdays/quieter days.

On the top, click **Options > Audio Status**

* Check the Input and Output Devices are set to Dante Virtual Soundcard
* Top left Power button needs to be blue - if it isn’t, click until it turns blue.

Presentation View of Pavilion 1

* Check the speakers are turning red when playing sound
* Check it says SHOW in big text underneath Output - if it says MUTE, the show is muted
* You can unmute the show in the Emergency Stop menu of Show Touch, or by clicking Output

**AUDIO SERVER 2 COMPUTER**

SAME AS AUDIO SERVER 1 except for Master volume control

**Troubleshooting:**

No sound coming out of speakers

* Check the show is unmuted
* Check the input and output in Audio Status
* Check the Power button in Audio Status is BLUE